**Existing Building Permit Form**

|  |  |
| --- | --- |
| Permit #: | Applicant Info: |
| Job Site Address: | Flood plain: |
| Historic Review: |  |

* In accordance with the International Existing Building Code (IEBC) Section 301.3, the applicant is required to provide the compliance path for review. Compliance methods shall not be applied in combination with each other.
* The general provisions for all compliance paths are found in Chapter 3 IEBC.

# Check the boxes the apply:

|  |  |
| --- | --- |
|  | Repair/voluntary structural retrofit |
|  | Alteration |
|  | Addition |
|  | Change of occupancy/use |
|  | Moved/relocated |

**Check one of the 4 paths below and each box under the path that applies: Repair/voluntary work only**

Structural damage to vertical elements of lateral force‐resisting system 405.2.3 IEBC Structural damage to gravity load‐carrying components 405.2.4 IEBC

Voluntary lateral force‐resisting system 503.13 IEBC

# Prescriptive compliance method Chapter 5 IEBC

Additions 502 IEBC

Alteration 503 IEBC

Change of occupancy 506 IEBC Accessibility 305 IEBC

Historic building 507 IEBC

# Work area compliance method Chapter 6‐12 IEBC

Alteration level I 602 IEBC Alteration level II 603 IEBC Alteration III 604 IEBC

Change of occupancy/use 605 IEBC Addition 606 IEBC

Accessibility 305 IEBC Historic building 607 IEBC

# Performance compliance method Chapter 13 IEBC (investigation/evaluation to be provided to the city for this method)

Fire safety, means of egress and general safety 1301 IEBC Structural analysis (required when using this path) 1301.4 IEBC Accessibility 305 IEBC