**Moisture Content & High-Efficiency Interior & Exterior Lighting System Acknowledgment Form**

CITY OF MEDFORD

Building Safety Department 200 S. Ivy Street

Medford, Oregon 97501

Phone: 541-774-2350

Email: building@cityofmedford.org Web: medfordoregon.gov/Home

I, , am the authorized agent or the owner at the following address:

Street Address

City State Zip Code

Permit #

1. R318.2 Moisture Content. Prior to the installation of interior finishes, the B*uilding Official* shall be notified in writing by the general contractor that all moisture-sensitive wood framing member used in construction have a moisture content of not more than 19 percent of the weight of dry wood framing members.
2. N1107.2 High-Efficiency Interior Lighting - All permanently installed lighting fixtures shall be high- efficiency light sources. The *building official* shall be notified in writing at the final inspection that the permanently installed lighting fixtures have met this requirement. Exception: Two permanently installed lighting fixtures are not required to be high-efficiency light sources when controlled by a dimmer or automatic control.
3. N1107.3 High-Efficiency Exterior Lighting – All exterior lighting fixtures affixed to the exterior of the building shall be high-efficiency light sources. Exception: Two permanently installed lighting fixtures are not required to be high-efficiency light sources when controlled by automatic control.

By signing below, I certify that I will meet the required minimums for the above mentioned building codes.

Print Name:

Signed: Date: (Circle One) Owner/General Contractor/Authorized Agent

P:\ADMIN\WEBSIE\OPENCITIES\WEBSITE FORMS\RESIDENTIAL PERMITS\Moisture Content